{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":37,"n_cols":5,"rows_kept":37,"merged":[[1,0,4,0],[5,0,6,0],[8,0,9,0],[12,0,15,0],[16,0,17,0],[18,0,19,0],[20,0,21,0],[22,0,23,0],[25,0,28,0],[29,0,30,0],[31,0,32,0],[33,0,34,0],[35,0,36,0]],"flags":["formulas_cached_only"]}
["区域","需求信息","DB地址"]
["一号入库站台","入库申请","DB3.0",null,"入库流程：当货物到达输送线终端入库口时，输送线给出入库请求信号、条码信息、重量信息，IWMS读取到之后生成任务回写确认信号，输送线清除这些请求"]
[null,"条码信息","DB3.6.0","50个字节,不足补空"]
[null,"重量信息","DB3.2","长整型，4字节"]
[null,"IWMS回写确认","DB3.0.1"]
["一号拣选工位（1）","拣选申请","DB3.58.0",null,"拣选流程：出入料箱到达拣选位之后，输送线扫描料箱条码，扫描完成后给出拣选请求及条码信息，IWMS读取后回写确认信号，输送线清除请求"]
[null,"条码信息","DB3.64.0","50个字节,不足补空"]
["一号拣选工位（1）拣选完成后箱子去向","箱子去向（流向：100流向库内，200料箱取出）WMS写入，PLC执行","DB3.60.0","100：PLC控制流向入库口\n200：PLC做什么处理？"]
["一号拣选工位（2）","拣选申请1","DB3.58.1"]
[null,"条码信息1","DB3.114","50个字节,不足补空"]
["一号拣选工位（2）拣选完成后箱子去向","箱子去向（流向：100流向库内，200料箱取出）WMS写入，PLC执行","DB3.62.0","100：PLC控制流向入库口\n200：PLC做什么处理？"]
[]
["二号入库站台","入库申请"]
[null,"条码信息"]
[null,"重量信息"]
[null,"IWMS回写确认"]
["二号拣选工位（1）","拣选申请"]
[null,"条码信息"]
["二号拣选工位（1）拣选完成后箱子去向","箱子去向（流向：100流向库内，200料箱取出）WMS写入，PLC执行"]
[null,"条码信息"]
["二号拣选工位（2）","拣选申请"]
[null,"条码信息"]
["二号拣选工位（2）拣选完成后箱子去向","箱子去向（流向：100流向库内，200料箱取出）WMS写入，PLC执行"]
[null,"条码信息"]
[]
["三号入库站台","入库申请"]
[null,"条码信息"]
[null,"重量信息"]
[null,"IWMS回写确认"]
["三号拣选工位（1）","拣选申请"]
[null,"条码信息"]
["三号拣选工位（1）拣选完成后箱子去向","箱子去向（流向：100流向库内，200料箱取出）WMS写入，PLC执行"]
[null,"条码信息"]
["三号拣选工位（2）","拣选申请"]
[null,"条码信息"]
["三号拣选工位（2）拣选完成后箱子去向","箱子去向（流向：100流向库内，200料箱取出）WMS写入，PLC执行"]
[null,"条码信息"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}