{"text_format":"3","workbook":"xls","n_sheets":5,"sheets":["烘箱、隔膜烘箱偏移地址对应关系","三楼负极分拨台、分拨台上料缓存线、隔膜工位偏移地址对应关系","三楼正极分拨台、分拨台上料缓存线、隔膜工位偏移地址对应关系","格林晟卷绕厂家提供变量地址","格林晟起始偏移地址对应关系"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"烘箱、隔膜烘箱偏移地址对应关系","index":0,"n_rows":98,"n_cols":20,"rows_kept":98,"merged":[[0,0,0,6],[2,0,13,0],[2,1,6,1],[2,7,13,7],[2,8,6,8],[2,14,13,14],[2,15,6,15],[8,1,13,1],[8,8,13,8],[8,15,13,15],[16,0,27,0],[16,1,20,1],[16,7,27,7],[16,8,20,8],[16,14,27,14],[16,15,20,15],[22,1,27,1],[22,8,27,8],[22,15,27,15],[30,0,41,0],[30,1,34,1],[30,7,41,7],[30,8,34,8],[30,14,41,14],[30,15,34,15],[36,1,41,1],[36,8,41,8],[36,15,41,15],[44,0,55,0],[44,1,48,1],[44,7,55,7],[44,8,48,8],[44,14,55,14],[44,15,48,15],[50,1,55,1],[50,8,55,8],[50,15,55,15],[58,0,69,0],[58,1,62,1],[58,7,69,7],[58,8,62,8],[58,14,69,14],[58,15,62,15],[64,1,69,1],[64,8,69,8],[64,15,69,15],[72,0,83,0],[72,1,76,1],[72,7,83,7],[72,8,76,8],[72,14,83,14],[72,15,76,15],[78,1,83,1],[78,8,83,8],[78,15,83,15],[86,0,97,0],[86,1,90,1],[86,7,97,7],[86,8,90,8],[92,1,97,1],[92,8,97,8]],"flags":["formulas_cached_only"]}
["注意：标黄部分为三楼正极AGV中控调度系统信号（192.168.11.87），未标黄部分\n为三楼负极AGV调度系统信号（192.168.11.88）"]
["烘箱IP地址",null,"读烘箱","写AGV","读AGV","写烘箱",null,"烘箱IP地址",null,"读烘箱","写AGV","读AGV","写烘箱",null,"烘箱IP地址",null,"读烘箱","写AGV","读AGV","写烘箱"]
["192.168.12.171","入料口","D1960","DB1002.1694.0","DB1002.1794.0","D1940",null,"192.168.12.172","入料口","D1960","DB1002.2094.0","DB1002.2194.0","D1940",null,"192.168.12.173","入料口","D1960","DB1002.2494.0","DB1002.2594.0","D1940"]
[null,null,"D15","DB1002.1695.0","DB1002.1795.0","D1941",{"$nulls":3},"D15","DB1002.2095.0","DB1002.2195.0","D1941",{"$nulls":3},"D15","DB1002.2495.0","DB1002.2595.0","D1941"]
[null,null,"D1961","DB1002.1696.0","DB1002.1796.0","D1955",{"$nulls":3},"D1961","DB1002.2096.0","DB1002.2196.0","D1955",{"$nulls":3},"D1961","DB1002.2496.0","DB1002.2596.0","D1955"]
[null,null,"D1950","DB1002.1697.0","DB1002.1797.0","D1956",{"$nulls":3},"D1950","DB1002.2097.0","DB1002.2197.0","D1956",{"$nulls":3},"D1950","DB1002.2497.0","DB1002.2597.0","D1956"]
[null,null,"D1951","DB1002.1698.0",{"$nulls":5},"D1951","DB1002.2098.0",{"$nulls":5},"D1951","DB1002.2498.0"]
[]
[null,"出料口","D1960","DB1002.294.0","DB1002.394.0","D1940",null,null,"出料口","D1960","DB1002.694.0","DB1002.794.0","D1940",null,null,"出料口","D1960","DB1002.1094.0","DB1002.1194.0","D1940"]
[null,null,"D35","DB1002.295.0","DB1002.395.0","D1941",{"$nulls":3},"D35","DB1002.695.0","DB1002.795.0","D1941",{"$nulls":3},"D35","DB1002.1095.0","DB1002.1195.0","D1941"]
[null,null,"D1962","DB1002.296.0","DB1002.396.0","D1957",{"$nulls":3},"D1962","DB1002.696.0","DB1002.796.0","D1957",{"$nulls":3},"D1962","DB1002.1096.0","DB1002.1196.0","D1957"]
[{"$nulls":4},"DB1002.397.0","D1952",{"$nulls":5},"DB1002.797.0","D1952",{"$nulls":5},"DB1002.1197.0","D1952"]
[{"$nulls":4},"DB1002.398.0","D1953",{"$nulls":5},"DB1002.798.0","D1953",{"$nulls":5},"DB1002.1198.0","D1953"]
[{"$nulls":4},"DB1002.399.0","D1958",{"$nulls":5},"DB1002.799.0","D1958",{"$nulls":5},"DB1002.1199.0","D1958"]
[]
["烘箱IP地址",null,"读烘箱","写AGV","读AGV","写烘箱",null,"烘箱IP地址",null,"读烘箱","写AGV","读AGV","写烘箱",null,"烘箱IP地址",null,"读烘箱","写AGV","读AGV","写烘箱"]
["192.168.12.174","入料口","D1960","DB1002.2894.0","DB1002.2994.0","D1940",null,"192.168.12.175","入料口","D1960","DB1002.3294.0","DB1002.3394.0","D1940",null,"192.168.12.176","入料口","D1960","DB1002.3694.0","DB1002.3794.0","D1940"]
[null,null,"D15","DB1002.2895.0","DB1002.2995.0","D1941",{"$nulls":3},"D15","DB1002.3295.0","DB1002.3395.0","D1941",{"$nulls":3},"D15","DB1002.3695.0","DB1002.3795.0","D1941"]
[null,null,"D1961","DB1002.2896.0","DB1002.2996.0","D1955",{"$nulls":3},"D1961","DB1002.3296.0","DB1002.3396.0","D1955",{"$nulls":3},"D1961","DB1002.3696.0","DB1002.3796.0","D1955"]
[null,null,"D1950","DB1002.2897.0","DB1002.2997.0","D1956",{"$nulls":3},"D1950","DB1002.3297.0","DB1002.3397.0","D1956",{"$nulls":3},"D1950","DB1002.3697.0","DB1002.3797.0","D1956"]
[null,null,"D1951","DB1002.2898.0",{"$nulls":5},"D1951","DB1002.3298.0",{"$nulls":5},"D1951","DB1002.3698.0"]
[]
[null,"出料口","D1960","DB1002.1494.0","DB1002.1594.0","D1940",null,null,"出料口","D1960","DB1002.1894.0","DB1002.1994.0","D1940",null,null,"出料口","D1960","DB1002.2294.0","DB1002.2394.0","D1940"]
[null,null,"D35","DB1002.1495.0","DB1002.1595.0","D1941",{"$nulls":3},"D35","DB1002.1895.0","DB1002.1995.0","D1941",{"$nulls":3},"D35","DB1002.2295.0","DB1002.2395.0","D1941"]
[null,null,"D1962","DB1002.1496.0","DB1002.1596.0","D1957",{"$nulls":3},"D1962","DB1002.1896.0","DB1002.1996.0","D1957",{"$nulls":3},"D1962","DB1002.2296.0","DB1002.2396.0","D1957"]
[{"$nulls":4},"DB1002.1597.0","D1952",{"$nulls":5},"DB1002.1997.0","D1952",{"$nulls":5},"DB1002.2397.0","D1952"]
[{"$nulls":4},"DB1002.1598.0","D1953",{"$nulls":5},"DB1002.1998.0","D1953",{"$nulls":5},"DB1002.2398.0","D1953"]
[{"$nulls":4},"DB1002.1599.0","D1958",{"$nulls":5},"DB1002.1999.0","D1958",{"$nulls":5},"DB1002.2399.0","D1958"]
[]
["烘箱IP地址",null,"读烘箱","写AGV","读AGV","写烘箱",null,"烘箱IP地址",null,"读烘箱","写AGV","读AGV","写烘箱",null,"烘箱IP地址",null,"读烘箱","写AGV","读AGV","写烘箱"]
["192.168.12.177","入料口","D1960","DB1002.4094.0","DB1002.4194.0","D1940",null,"192.168.12.178","入料口","D1960","DB1002.4494.0","DB1002.4594.0","D1940",null,"192.168.12.181","入料口","D1960","DB1002.4894.0","DB1002.4994.0","D1940"]
[null,null,"D15","DB1002.4095.0","DB1002.4195.0","D1941",{"$nulls":3},"D15","DB1002.4495.0","DB1002.4595.0","D1941",{"$nulls":3},"D15","DB1002.4895.0","DB1002.4995.0","D1941"]
[null,null,"D1961","DB1002.4096.0","DB1002.4196.0","D1955",{"$nulls":3},"D1961","DB1002.4496.0","DB1002.4596.0","D1955",{"$nulls":3},"D1961","DB1002.4896.0","DB1002.4996.0","D1955"]
[null,null,"D1950","DB1002.4097.0","DB1002.4197.0","D1956",{"$nulls":3},"D1950","DB1002.4497.0","DB1002.4597.0","D1956",{"$nulls":3},"D1950","DB1002.4897.0","DB1002.4997.0","D1956"]
[null,null,"D1951","DB1002.4098.0",{"$nulls":5},"D1951","DB1002.4498.0",{"$nulls":5},"D1951","DB1002.4898.0"]
[]
[null,"出料口","D1960","DB1002.2694.0","DB1002.2794.0","D1940",null,null,"出料口","D1960","DB1002.3094.0","DB1002.3194.0","D1940",null,null,"出料口","D1960","DB1002.5094.0","DB1002.5194.0","D1940"]
[null,null,"D35","DB1002.2695.0","DB1002.2795.0","D1941",{"$nulls":3},"D35","DB1002.3095.0","DB1002.3195.0","D1941",{"$nulls":3},"D35","DB1002.5095.0","DB1002.5195.0","D1941"]
[null,null,"D1962","DB1002.2696.0","DB1002.2796.0","D1957",{"$nulls":3},"D1962","DB1002.3096.0","DB1002.3196.0","D1957",{"$nulls":3},"D1962","DB1002.5096.0","DB1002.5196.0","D1957"]
[{"$nulls":4},"DB1002.2797.0","D1952",{"$nulls":5},"DB1002.3197.0","D1952",{"$nulls":5},"DB1002.5197.0","D1952"]
[{"$nulls":4},"DB1002.2798.0","D1953",{"$nulls":5},"DB1002.3198.0","D1953",{"$nulls":5},"DB1002.5198.0","D1953"]
[{"$nulls":4},"DB1002.2799.0","D1958",{"$nulls":5},"DB1002.3199.0","D1958",{"$nulls":5},"DB1002.5199.0","D1958"]
[]
["烘箱IP地址",null,"读烘箱","写AGV","读AGV","写烘箱",null,"烘箱IP地址",null,"读烘箱","写AGV","读AGV","写烘箱",null,"烘箱IP地址",null,"读烘箱","写AGV","读AGV","写烘箱"]
["192.168.12.182","入料口","D1960","DB1002.5294.0","DB1002.5394.0","D1940",null,"192.168.12.183","入料口","D1960","DB1002.5694.0","DB1002.5794.0","D1940",null,"192.168.12.184","入料口","D1960","DB1002.6094.0","DB1002.6194.0","D1940"]
[null,null,"D15","DB1002.5295.0","DB1002.5395.0","D1941",{"$nulls":3},"D15","DB1002.5695.0","DB1002.5795.0","D1941",{"$nulls":3},"D15","DB1002.6095.0","DB1002.6195.0","D1941"]
[null,null,"D1961","DB1002.5296.0","DB1002.5396.0","D1955",{"$nulls":3},"D1961","DB1002.5696.0","DB1002.5796.0","D1955",{"$nulls":3},"D1961","DB1002.6096.0","DB1002.6196.0","D1955"]
[null,null,"D1950","DB1002.5297.0","DB1002.5397.0","D1956",{"$nulls":3},"D1950","DB1002.5697.0","DB1002.5797.0","D1956",{"$nulls":3},"D1950","DB1002.6097.0","DB1002.6197.0","D1956"]
[null,null,"D1951","DB1002.5298.0",{"$nulls":5},"D1951","DB1002.5698.0",{"$nulls":5},"D1951","DB1002.6098.0"]
[]
[null,"出料口","D1960","DB1002.5494.0","DB1002.5594.0","D1940",null,null,"出料口","D1960","DB1002.5894.0","DB1002.5994.0","D1940",null,null,"出料口","D1960","DB1002.6294.0","DB1002.6394.0","D1940"]
[null,null,"D35","DB1002.5495.0","DB1002.5595.0","D1941",{"$nulls":3},"D35","DB1002.5895.0","DB1002.5995.0","D1941",{"$nulls":3},"D35","DB1002.6295.0","DB1002.6395.0","D1941"]
[null,null,"D1962","DB1002.5496.0","DB1002.5596.0","D1957",{"$nulls":3},"D1962","DB1002.5896.0","DB1002.5996.0","D1957",{"$nulls":3},"D1962","DB1002.6296.0","DB1002.6396.0","D1957"]
[{"$nulls":4},"DB1002.5597.0","D1952",{"$nulls":5},"DB1002.5997.0","D1952",{"$nulls":5},"DB1002.6397.0","D1952"]
[{"$nulls":4},"DB1002.5598.0","D1953",{"$nulls":5},"DB1002.5998.0","D1953",{"$nulls":5},"DB1002.6398.0","D1953"]
[{"$nulls":4},"DB1002.5599.0","D1958",{"$nulls":5},"DB1002.5999.0","D1958",{"$nulls":5},"DB1002.6399.0","D1958"]
[]
["烘箱IP地址",null,"读烘箱","写AGV","读AGV","写烘箱",null,"烘箱IP地址",null,"读烘箱","写AGV","读AGV","写烘箱",null,"烘箱IP地址",null,"读烘箱","写AGV","读AGV","写烘箱"]
["192.168.12.185","入料口","D1960","DB1002.6494.0","DB1002.6594.0","D1940",null,"192.168.12.186","入料口","D1960","DB1002.6894.0","DB1002.6994.0","D1940",null,"192.168.12.187","入料口","D1960","DB1002.7294.0","DB1002.7394.0","D1940"]
[null,null,"D15","DB1002.6495.0","DB1002.6595.0","D1941",{"$nulls":3},"D15","DB1002.6895.0","DB1002.6995.0","D1941",{"$nulls":3},"D15","DB1002.7295.0","DB1002.7395.0","D1941"]
[null,null,"D1961","DB1002.6496.0","DB1002.6596.0","D1955",{"$nulls":3},"D1961","DB1002.6896.0","DB1002.6996.0","D1955",{"$nulls":3},"D1961","DB1002.7296.0","DB1002.7396.0","D1955"]
[null,null,"D1950","DB1002.6497.0","DB1002.6597.0","D1956",{"$nulls":3},"D1950","DB1002.6897.0","DB1002.6997.0","D1956",{"$nulls":3},"D1950","DB1002.7297.0","DB1002.7397.0","D1956"]
[null,null,"D1951","DB1002.6498.0",{"$nulls":5},"D1951","DB1002.6898.0",{"$nulls":5},"D1951","DB1002.7298.0"]
[]
[null,"出料口","D1960","DB1002.6694.0","DB1002.6794.0","D1940",null,null,"出料口","D1960","DB1002.7094.0","DB1002.7194.0","D1940",null,null,"出料口","D1960","DB1002.7494.0","DB1002.7594.0","D1940"]
[null,null,"D35","DB1002.6695.0","DB1002.6795.0","D1941",{"$nulls":3},"D35","DB1002.7095.0","DB1002.7195.0","D1941",{"$nulls":3},"D35","DB1002.7495.0","DB1002.7595.0","D1941"]
[null,null,"D1962","DB1002.6696.0","DB1002.6796.0","D1957",{"$nulls":3},"D1962","DB1002.7096.0","DB1002.7196.0","D1957",{"$nulls":3},"D1962","DB1002.7496.0","DB1002.7596.0","D1957"]
[{"$nulls":4},"DB1002.6797.0","D1952",{"$nulls":5},"DB1002.7197.0","D1952",{"$nulls":5},"DB1002.7597.0","D1952"]
[{"$nulls":4},"DB1002.6798.0","D1953",{"$nulls":5},"DB1002.7198.0","D1953",{"$nulls":5},"DB1002.7598.0","D1953"]
[{"$nulls":4},"DB1002.6799.0","D1958",{"$nulls":5},"DB1002.7199.0","D1958",{"$nulls":5},"DB1002.7599.0","D1958"]
[]
["烘箱IP地址",null,"读烘箱","写AGV","读AGV","写烘箱",null,"烘箱IP地址",null,"读烘箱","写AGV","读AGV","写烘箱",null,"烘箱IP地址",null,"读烘箱","写AGV","读AGV","写烘箱"]
["192.168.12.188","入料口","D1960","DB1002.7694.0","DB1002.7794.0","D1940",null,"192.168.12.169","入料口","D1960","DB1002.8094.0","DB1002.8194.0","D1940",null,"192.168.12.170","入料口","D1960","DB1002.8494.0","DB1002.8594.0","D1940"]
[null,null,"D15","DB1002.7695.0","DB1002.7795.0","D1941",{"$nulls":3},"D15","DB1002.8095.0","DB1002.8195.0","D1941",{"$nulls":3},"D15","DB1002.8495.0","DB1002.8595.0","D1941"]
[null,null,"D1961","DB1002.7696.0","DB1002.7796.0","D1955",{"$nulls":3},"D1961","DB1002.8096.0","DB1002.8196.0","D1955",{"$nulls":3},"D1961","DB1002.8496.0","DB1002.8596.0","D1955"]
[null,null,"D1950","DB1002.7697.0","DB1002.7797.0","D1956",{"$nulls":3},"D1950","DB1002.8097.0","DB1002.8197.0","D1956",{"$nulls":3},"D1950","DB1002.8497.0","DB1002.8597.0","D1956"]
[null,null,"D1951","DB1002.7698.0",{"$nulls":5},"D1951","DB1002.8098.0",{"$nulls":5},"D1951","DB1002.8498.0"]
[]
[null,"出料口","D1960","DB1002.7894.0","DB1002.7994.0","D1940",null,null,"出料口","D1960","DB1002.3494.0","DB1002.3594.0","D1940",null,null,"出料口","D1960","DB1002.3894.0","DB1002.3994.0","D1940"]
[null,null,"D35","DB1002.7895.0","DB1002.7995.0","D1941",{"$nulls":3},"D35","DB1002.3495.0","DB1002.3595.0","D1941",{"$nulls":3},"D35","DB1002.3895.0","DB1002.3995.0","D1941"]
[null,null,"D1962","DB1002.7896.0","DB1002.7996.0","D1957",{"$nulls":3},"D1962","DB1002.3496.0","DB1002.3596.0","D1957",{"$nulls":3},"D1962","DB1002.3896.0","DB1002.3996.0","D1957"]
[{"$nulls":4},"DB1002.7997.0","D1952",{"$nulls":5},"DB1002.3597.0","D1952",{"$nulls":5},"DB1002.3997.0","D1952"]
[{"$nulls":4},"DB1002.7998.0","D1953",{"$nulls":5},"DB1002.3598.0","D1953",{"$nulls":5},"DB1002.3998.0","D1953"]
[{"$nulls":4},"DB1002.7999.0","D1958",{"$nulls":5},"DB1002.3599.0","D1958",{"$nulls":5},"DB1002.3999.0","D1958"]
[]
["烘箱IP地址",null,"读烘箱","写AGV","读AGV","写烘箱",null,"烘箱IP地址",null,"读烘箱","写AGV","读AGV","写烘箱"]
["192.168.12.179","入料口","D1960","DB1002.8894.0","DB1002.8994.0","D1940",null,"192.168.12.180","入料口","D1960","DB1002.9294.0","DB1002.9394.0","D1940"]
[null,null,"D15","DB1002.8895.0","DB1002.8995.0","D1941",{"$nulls":3},"D15","DB1002.9295.0","DB1002.9395.0","D1941"]
[null,null,"D1961","DB1002.8896.0","DB1002.8996.0","D1955",{"$nulls":3},"D1961","DB1002.9296.0","DB1002.9396.0","D1955"]
[null,null,"D1950","DB1002.8897.0","DB1002.8997.0","D1956",{"$nulls":3},"D1950","DB1002.9297.0","DB1002.9397.0","D1956"]
[null,null,"D1951","DB1002.8898.0",{"$nulls":5},"D1951","DB1002.9298.0"]
[]
[null,"出料口","D1960","DB1002.9094.0","DB1002.9194.0","D1940",null,null,"出料口","D1960","DB1002.9494.0","DB1002.9594.0","D1940"]
[null,null,"D35","DB1002.9095.0","DB1002.9195.0","D1941",{"$nulls":3},"D35","DB1002.9495.0","DB1002.9595.0","D1941"]
[null,null,"D1962","DB1002.9096.0","DB1002.9196.0","D1957",{"$nulls":3},"D1962","DB1002.9496.0","DB1002.9596.0","D1957"]
[{"$nulls":4},"DB1002.9197.0","D1952",{"$nulls":5},"DB1002.9597.0","D1952"]
[{"$nulls":4},"DB1002.9198.0","D1953",{"$nulls":5},"DB1002.9598.0","D1953"]
[{"$nulls":4},"DB1002.9199.0","D1958",{"$nulls":5},"DB1002.9599.0","D1958"]

{"sheet":"三楼负极分拨台、分拨台上料缓存线、隔膜工位偏移地址对应关系","index":1,"n_rows":27,"n_cols":13,"rows_kept":27,"merged":[[1,0,2,0],[1,7,2,7],[3,0,18,0],[3,7,18,7],[19,0,26,0]],"flags":["formulas_cached_only"]}
["西门子1200","读PLC(192.168.11.194)","写AGV中控(三楼负极中控192.168.11.88)","读AGV中控","写PLC","数据长度",null,"西门子1200","读PLC(192.168.11.188)","写AGV中控(三楼负极中控192.168.11.88)","读AGV中控","写PLC","数据长度"]
["分拨台","DB100.0.0","DB1002.26000.0","DB1002.26100.0","DB200.0.0","100BYTE",null,"分拨台","DB100.0.0","DB1002.25600.0","DB1002.25700.0","DB200.0.0","100BYTE"]
[null,"DB100.100.0","DB1002.26200.0","DB1002.26300.0","DB200.100.0","100BYTE",null,null,"DB100.100.0","DB1002.25800.0","DB1002.25900.0","DB200.100.0","100BYTE"]
["分拨台上料缓存线","DB100.200.0","DB1002.22400.0","DB1002.22500.0","DB200.200.0","100BYTE",null,"分拨台上料缓存线","DB100.200.0","DB1002.19200.0","DB1002.19300.0","DB200.200.0","100BYTE"]
[null,"DB100.300.0","DB1002.22600.0","DB1002.22700.0","DB200.300.0","100BYTE",null,null,"DB100.300.0","DB1002.19400.0","DB1002.19500.0","DB200.300.0","100BYTE"]
[null,"DB100.400.0","DB1002.22800.0","DB1002.22900.0","DB200.400.0","100BYTE",null,null,"DB100.400.0","DB1002.19600.0","DB1002.19700.0","DB200.400.0","100BYTE"]
[null,"DB100.500.0","DB1002.23000.0","DB1002.23100.0","DB200.500.0","100BYTE",null,null,"DB100.500.0","DB1002.19800.0","DB1002.19900.0","DB200.500.0","100BYTE"]
[null,"DB100.600.0","DB1002.23200.0","DB1002.23300.0","DB200.600.0","100BYTE",null,null,"DB100.600.0","DB1002.20000.0","DB1002.20100.0","DB200.600.0","100BYTE"]
[null,"DB100.700.0","DB1002.23400.0","DB1002.23500.0","DB200.700.0","100BYTE",null,null,"DB100.700.0","DB1002.20200.0","DB1002.20300.0","DB200.700.0","100BYTE"]
[null,"DB100.800.0","DB1002.23600.0","DB1002.23700.0","DB200.800.0","100BYTE",null,null,"DB100.800.0","DB1002.20400.0","DB1002.20500.0","DB200.800.0","100BYTE"]
[null,"DB100.900.0","DB1002.23800.0","DB1002.23900.0","DB200.900.0","100BYTE",null,null,"DB100.900.0","DB1002.20600.0","DB1002.20700.0","DB200.900.0","100BYTE"]
[null,"DB100.1000.0","DB1002.24000.0","DB1002.24100.0","DB200.1000.0","100BYTE",null,null,"DB100.1000.0","DB1002.20800.0","DB1002.20900.0","DB200.1000.0","100BYTE"]
[null,"DB100.1100.0","DB1002.24200.0","DB1002.24300.0","DB200.1100.0","100BYTE",null,null,"DB100.1100.0","DB1002.21000.0","DB1002.21100.0","DB200.1100.0","100BYTE"]
[null,"DB100.1200.0","DB1002.24400.0","DB1002.24500.0","DB200.1200.0","100BYTE",null,null,"DB100.1200.0","DB1002.21200.0","DB1002.21300.0","DB200.1200.0","100BYTE"]
[null,"DB100.1300.0","DB1002.24600.0","DB1002.24700.0","DB200.1300.0","100BYTE",null,null,"DB100.1300.0","DB1002.21400.0","DB1002.21500.0","DB200.1300.0","100BYTE"]
[null,"DB100.1400.0","DB1002.24800.0","DB1002.24900.0","DB200.1400.0","100BYTE",null,null,"DB100.1400.0","DB1002.21600.0","DB1002.21700.0","DB200.1400.0","100BYTE"]
[null,"DB100.1500.0","DB1002.25000.0","DB1002.25100.0","DB200.1500.0","100BYTE",null,null,"DB100.1500.0","DB1002.21800.0","DB1002.21900.0","DB200.1500.0","100BYTE"]
[null,"DB100.1600.0","DB1002.25200.0","DB1002.25300.0","DB200.1600.0","100BYTE",null,null,"DB100.1600.0","DB1002.22000.0","DB1002.22100.0","DB200.1600.0","100BYTE"]
[null,"DB100.1700.0","DB1002.25400.0","DB1002.25500.0","DB200.1700.0","100BYTE",null,null,"DB100.1700.0","DB1002.22200.0","DB1002.22300.0","DB200.1700.0","100BYTE"]
["隔膜工位","DB100.1800.0","DB1002.26400.0","DB1002.26500.0","DB200.1800.0","100BYTE"]
[null,"DB100.1900.0","DB1002.26600.0","DB1002.26700.0","DB200.1900.0","100BYTE"]
[null,"DB100.2000.0","DB1002.26800.0","DB1002.26900.0","DB200.2000.0","100BYTE"]
[null,"DB100.2100.0","DB1002.27000.0","DB1002.27100.0","DB200.2100.0","100BYTE"]
[null,"DB100.2200.0","DB1002.27200.0","DB1002.27300.0","DB200.2200.0","100BYTE"]
[null,"DB100.2300.0","DB1002.27400.0","DB1002.27500.0","DB200.2300.0","100BYTE"]
[null,"DB100.2400.0","DB1002.27600.0","DB1002.27700.0","DB200.2400.0","100BYTE"]
[null,"DB100.2500.0","DB1002.27800.0","DB1002.27900.0","DB200.2500.0","100BYTE"]

{"sheet":"三楼正极分拨台、分拨台上料缓存线、隔膜工位偏移地址对应关系","index":2,"n_rows":27,"n_cols":13,"rows_kept":27,"merged":[[1,0,2,0],[1,7,2,7],[3,0,18,0],[3,7,18,7],[19,0,26,0]],"flags":["formulas_cached_only"]}
["西门子1200","读PLC(192.168.11.176)","写AGV中控(三楼正极中控192.168.11.87)","读AGV中控","写PLC","数据长度",null,"西门子1200","读PLC(192.168.11.182)","写AGV中控(三楼正极中控192.168.11.87)","读AGV中控","写PLC","数据长度"]
["分拨台","DB100.0.0","DB1002.10800.0","DB1002.10900.0","DB200.0.0","100BYTE",null,"分拨台","DB100.0.0","DB1002.11200.0","DB1002.11300.0","DB200.0.0","100BYTE"]
[null,"DB100.100.0","DB1002.11000.0","DB1002.11100.0","DB200.100.0","100BYTE",null,null,"DB100.100.0","DB1002.11400.0","DB1002.11500.0","DB200.100.0","100BYTE"]
["分拨台上料缓存线","DB100.200.0","DB1002.4400.0","DB1002.4500.0","DB200.200.0","100BYTE",null,"分拨台上料缓存线","DB100.200.0","DB1002.7600.0","DB1002.7700.0","DB200.200.0","100BYTE"]
[null,"DB100.300.0","DB1002.4600.0","DB1002.4700.0","DB200.300.0","100BYTE",null,null,"DB100.300.0","DB1002.7800.0","DB1002.7900.0","DB200.300.0","100BYTE"]
[null,"DB100.400.0","DB1002.4800.0","DB1002.4900.0","DB200.400.0","100BYTE",null,null,"DB100.400.0","DB1002.8000.0","DB1002.8100.0","DB200.400.0","100BYTE"]
[null,"DB100.500.0","DB1002.5000.0","DB1002.5100.0","DB200.500.0","100BYTE",null,null,"DB100.500.0","DB1002.8200.0","DB1002.8300.0","DB200.500.0","100BYTE"]
[null,"DB100.600.0","DB1002.5200.0","DB1002.5300.0","DB200.600.0","100BYTE",null,null,"DB100.600.0","DB1002.8400.0","DB1002.8500.0","DB200.600.0","100BYTE"]
[null,"DB100.700.0","DB1002.5400.0","DB1002.5500.0","DB200.700.0","100BYTE",null,null,"DB100.700.0","DB1002.8600.0","DB1002.8700.0","DB200.700.0","100BYTE"]
[null,"DB100.800.0","DB1002.5600.0","DB1002.5700.0","DB200.800.0","100BYTE",null,null,"DB100.800.0","DB1002.8800.0","DB1002.8900.0","DB200.800.0","100BYTE"]
[null,"DB100.900.0","DB1002.5800.0","DB1002.5900.0","DB200.900.0","100BYTE",null,null,"DB100.900.0","DB1002.9000.0","DB1002.9100.0","DB200.900.0","100BYTE"]
[null,"DB100.1000.0","DB1002.6000.0","DB1002.6100.0","DB200.1000.0","100BYTE",null,null,"DB100.1000.0","DB1002.9200.0","DB1002.9300.0","DB200.1000.0","100BYTE"]
[null,"DB100.1100.0","DB1002.6200.0","DB1002.6300.0","DB200.1100.0","100BYTE",null,null,"DB100.1100.0","DB1002.9400.0","DB1002.9500.0","DB200.1100.0","100BYTE"]
[null,"DB100.1200.0","DB1002.6400.0","DB1002.6500.0","DB200.1200.0","100BYTE",null,null,"DB100.1200.0","DB1002.9600.0","DB1002.9700.0","DB200.1200.0","100BYTE"]
[null,"DB100.1300.0","DB1002.6600.0","DB1002.6700.0","DB200.1300.0","100BYTE",null,null,"DB100.1300.0","DB1002.9800.0","DB1002.9900.0","DB200.1300.0","100BYTE"]
[null,"DB100.1400.0","DB1002.6800.0","DB1002.6900.0","DB200.1400.0","100BYTE",null,null,"DB100.1400.0","DB1002.10000.0","DB1002.10100.0","DB200.1400.0","100BYTE"]
[null,"DB100.1500.0","DB1002.7000.0","DB1002.7100.0","DB200.1500.0","100BYTE",null,null,"DB100.1500.0","DB1002.10200.0","DB1002.10300.0","DB200.1500.0","100BYTE"]
[null,"DB100.1600.0","DB1002.7200.0","DB1002.7300.0","DB200.1600.0","100BYTE",null,null,"DB100.1600.0","DB1002.10400.0","DB1002.10500.0","DB200.1600.0","100BYTE"]
[null,"DB100.1700.0","DB1002.7400.0","DB1002.7500.0","DB200.1700.0","100BYTE",null,null,"DB100.1700.0","DB1002.10600.0","DB1002.10700.0","DB200.1700.0","100BYTE"]
["隔膜工位","DB100.1800.0","DB1002.11600.0","DB1002.11700.0","DB200.1800.0","100BYTE"]
[null,"DB100.1900.0","DB1002.11800.0","DB1002.11900.0","DB200.1900.0","100BYTE"]
[null,"DB100.2000.0","DB1002.12000.0","DB1002.12100.0","DB200.2000.0","100BYTE"]
[null,"DB100.2100.0","DB1002.12200.0","DB1002.12300.0","DB200.2100.0","100BYTE"]
[null,"DB100.2200.0","DB1002.12400.0","DB1002.12500.0","DB200.2200.0","100BYTE"]
[null,"DB100.2300.0","DB1002.12600.0","DB1002.12700.0","DB200.2300.0","100BYTE"]
[null,"DB100.2400.0","DB1002.12800.0","DB1002.12900.0","DB200.2400.0","100BYTE"]
[null,"DB100.2500.0","DB1002.13000.0","DB1002.13100.0","DB200.2500.0","100BYTE"]

{"sheet":"格林晟卷绕厂家提供变量地址","index":3,"n_rows":83,"n_cols":5,"rows_kept":83,"flags":["formulas_cached_only"]}
["补充备注：工单号地址：D2661","STRING[256]"]
[]
["信号名称","变量类型","PLC地址","信号方向","信号说明"]
["心跳位","Bool","D2920","设备—>调度","当收到调度心跳原样返回"]
["对接设备编号","String[20]","D2922","设备—>调度"]
["入料口任务需求类型（左极左放卷）","UInt","D2923","设备—>调度","0-无需求，1进料，2-出料"]
["入料口需求的容器物料编码（左极左放卷）","String[30]","D2924","设备—>调度"]
["预留点位（左极左放卷）","String[30]","D2925","设备—>调度"]
["入料口设备对接流程步骤（左极左放卷）","Int","D2926","设备—>调度"]
["预留点位（左极左放卷）","Int","D2927","设备—>调度"]
["入料口设备对接报警（左极左放卷）","Bool","D2928","设备—>调度","0：无报警，1：报警在报警状态下，AGV将不接收作业请求,对接中报警AGV将停止一切对接动作等待人工处理。"]
["预留点位（左极左放卷）","Bool","D2929","设备—>调度"]
["入料口设备对接请求（左极左放卷）","Bool","D2930","设备—>调度","设备发起请求，AGV调度系统产生任务"]
["预留点位（左极左放卷）","Bool","D2931","设备—>调度"]
["预留点位（左极左放卷）","Bool","D2932","设备—>调度"]
["预留点位（左极左放卷）","Bool","D2933","设备—>调度"]
[]
["入料口任务需求类型（左极右放卷）","UInt","D2934","设备—>调度","0-无需求，1进料，2-出料"]
["入料口需求的容器物料编码（左极右放卷）","String[30]","D2935","设备—>调度"]
["预留点位（左极右放卷）","String[30]","D2936","设备—>调度"]
["入料口设备对接流程步骤（左极右放卷）","Int","D2937","设备—>调度"]
["预留点位（左极右放卷）","Int","D2938","设备—>调度"]
["入料口设备对接报警（左极右放卷）","Bool","D2939","设备—>调度","0：无报警，1：报警在报警状态下，AGV将不接收作业请求,对接中报警AGV将停止一切对接动作等待人工处理。"]
["预留点位（左极右放卷）","Bool","D2940","设备—>调度"]
["入料口设备对接请求（左极右放卷）","Bool","D2941","设备—>调度","设备发起请求，AGV调度系统产生任务"]
["预留点位（左极右放卷）","Bool","D2942","设备—>调度"]
["预留点位（左极右放卷）","Bool","D2943","设备—>调度"]
["预留点位（左极右放卷）","Bool","D2944","设备—>调度"]
[]
["入料口任务需求类型（右极左放卷）","UInt","D2945","设备—>调度","0-无需求，1进料，2-出料"]
["入料口需求的容器物料编码（右极左放卷）","String[30]","D2946","设备—>调度"]
["预留点位（右极左放卷）","String[30]","D2947","设备—>调度"]
["入料口设备对接流程步骤（右极左放卷）","Int","D2948","设备—>调度"]
["预留点位（右极左放卷）","Int","D2949","设备—>调度"]
["入料口设备对接报警（右极左放卷）","Bool","D2950","设备—>调度","0：无报警，1：报警在报警状态下，AGV将不接收作业请求,对接中报警AGV将停止一切对接动作等待人工处理。"]
["预留点位（右极左放卷）","Bool","D2951","设备—>调度"]
["入料口设备对接请求（右极左放卷）","Bool","D2952","设备—>调度","设备发起请求，AGV调度系统产生任务"]
["预留点位（右极左放卷）","Bool","D2953","设备—>调度"]
["预留点位（右极左放卷）","Bool","D2954","设备—>调度"]
["预留点位（右极左放卷）","Bool","D2955","设备—>调度"]
[]
["入料口任务需求类型（右极右放卷）","UInt","D2956","设备—>调度","0-无需求，1进料，2-出料"]
["入料口需求的容器物料编码（右极右放卷）","String[30]","D2957","设备—>调度"]
["预留点位（右极右放卷）","String[30]","D2958","设备—>调度"]
["入料口设备对接流程步骤（右极右放卷）","Int","D2959","设备—>调度"]
["预留点位（右极右放卷）","Int","D2960","设备—>调度"]
["入料口设备对接报警（右极右放卷）","Bool","D2961","设备—>调度","0：无报警，1：报警在报警状态下，AGV将不接收作业请求,对接中报警AGV将停止一切对接动作等待人工处理。"]
["预留点位（右极右放卷）","Bool","D2962","设备—>调度"]
["入料口设备对接请求（右极右放卷）","Bool","D2963","设备—>调度","设备发起请求，AGV调度系统产生任务"]
["预留点位（右极右放卷）","Bool","D2964","设备—>调度"]
["预留点位（右极右放卷）","Bool","D2965","设备—>调度"]
["预留点位（右极右放卷）","Bool","D2966","设备—>调度"]
[]
["信号名称","变量类型","PLC地址","信号方向","信号说明"]
["心跳位","Bool","D2970","调度—>设备","当收到设备心跳取反位发送"]
["预留点位","String[20]","D2972","调度—>设备"]
["预留点位（左极左放卷）","UInt","D2973","调度—>设备"]
["预留点位（左极左放卷）","String[30]","D2974","调度—>设备"]
["入料口AGV对接流程步骤（左极左放卷）","Int","D2975","调度—>设备"]
["预留点位（左极左放卷）","Int","D2976","调度—>设备"]
["入料口AGV对接报警（左极左放卷）","Bool","D2977","调度—>设备"]
["预留点位（左极左放卷）","Bool","D2978","调度—>设备"]
[]
["预留点位（左极右放卷）","UInt","D2979","调度—>设备"]
["预留点位（左极右放卷）","String[30]","D2980","调度—>设备"]
["入料口AGV对接流程步骤（左极右放卷）","Int","D2981","调度—>设备"]
["预留点位（左极右放卷）","Int","D2982","调度—>设备"]
["入料口AGV对接报警（左极右放卷）","Bool","D2983","调度—>设备"]
["预留点位（左极右放卷）","Bool","D2984","调度—>设备"]
[]
["预留点位（右极左放卷）","UInt","D2985","调度—>设备"]
["预留点位（右极左放卷）","String[30]","D2986","调度—>设备"]
["入料口AGV对接流程步骤（右极左放卷）","Int","D2987","调度—>设备"]
["预留点位（右极左放卷）","Int","D2988","调度—>设备"]
["入料口AGV对接报警（右极左放卷）","Bool","D2989","调度—>设备"]
["预留点位（右极左放卷）","Bool","D2990","调度—>设备"]
[]
["预留点位（右极右放卷）","UInt","D2991","调度—>设备"]
["预留点位（右极右放卷）","String[30]","D2992","调度—>设备"]
["入料口AGV对接流程步骤（右极右放卷）","Int","D2993","调度—>设备"]
["预留点位（右极右放卷）","Int","D2994","调度—>设备"]
["入料口AGV对接报警（右极右放卷）","Bool","D2995","调度—>设备"]
["预留点位（右极右放卷）","Bool","D2996","调度—>设备"]

{"sheet":"格林晟起始偏移地址对应关系","index":4,"n_rows":34,"n_cols":11,"rows_kept":34,"merged":[[1,0,5,0],[1,6,5,6],[8,0,12,0],[8,6,12,6],[15,0,19,0],[15,6,19,6],[22,0,26,0],[22,6,26,6],[29,0,33,0],[29,6,33,6]],"flags":["formulas_cached_only"]}
[]
["192.168.12.189","读格林晟","写AGV(三楼负极中控 192.168.11.88)","读AGV","写格林晟",null,"192.168.12.194","读格林晟","写AGV(三楼负极中控 192.168.11.88)","读AGV","写格林晟"]
[null,"D2920","DB1002.9600.0","DB1002.9700.0","D2970",null,null,"D2920","DB1002.13600.0","DB1002.13700.0","D2970"]
[null,"D2934","DB1002.9800.0","DB1002.9900.0","D2979",null,null,"D2934","DB1002.13800.0","DB1002.13900.0","D2979"]
[null,"D2945","DB1002.10000.0","DB1002.10100.0","D2985",null,null,"D2945","DB1002.14000.0","DB1002.14100.0","D2985"]
[null,"D2956","DB1002.10200.0","DB1002.10300.0","D2991",null,null,"D2956","DB1002.14200.0","DB1002.14300.0","D2991"]
[]
[]
["192.168.12.190","读格林晟","写AGV(三楼负极中控 192.168.11.88)","读AGV","写格林晟",null,"192.168.12.195","读格林晟","写AGV(三楼负极中控 192.168.11.88)","读AGV","写格林晟"]
[null,"D2920","DB1002.10400.0","DB1002.10500.0","D2970",null,null,"D2920","DB1002.14400.0","DB1002.14500.0","D2970"]
[null,"D2934","DB1002.10600.0","DB1002.10700.0","D2979",null,null,"D2934","DB1002.14600.0","DB1002.14700.0","D2979"]
[null,"D2945","DB1002.10800.0","DB1002.10900.0","D2985",null,null,"D2945","DB1002.14800.0","DB1002.14900.0","D2985"]
[null,"D2956","DB1002.11000.0","DB1002.11100.0","D2991",null,null,"D2956","DB1002.15000.0","DB1002.15100.0","D2991"]
[]
[]
["192.168.12.191","读格林晟","写AGV(三楼负极中控 192.168.11.88)","读AGV","写格林晟",null,"192.168.12.196","读格林晟","写AGV(三楼负极中控 192.168.11.88)","读AGV","写格林晟"]
[null,"D2920","DB1002.11200.0","DB1002.11300.0","D2970",null,null,"D2920","DB1002.15200.0","DB1002.15300.0","D2970"]
[null,"D2934","DB1002.11400.0","DB1002.11500.0","D2979",null,null,"D2934","DB1002.15400.0","DB1002.15500.0","D2979"]
[null,"D2945","DB1002.11600.0","DB1002.11700.0","D2985",null,null,"D2945","DB1002.15600.0","DB1002.15700.0","D2985"]
[null,"D2956","DB1002.11800.0","DB1002.11900.0","D2991",null,null,"D2956","DB1002.15800.0","DB1002.15900.0","D2991"]
[]
[]
["192.168.12.192","读格林晟","写AGV(三楼负极中控 192.168.11.88)","读AGV","写格林晟",null,"192.168.12.197","读格林晟","写AGV(三楼负极中控 192.168.11.88)","读AGV","写格林晟"]
[null,"D2920","DB1002.12000.0","DB1002.12100.0","D2970",null,null,"D2920","DB1002.16000.0","DB1002.16100.0","D2970"]
[null,"D2934","DB1002.12200.0","DB1002.12300.0","D2979",null,null,"D2934","DB1002.16200.0","DB1002.16300.0","D2979"]
[null,"D2945","DB1002.12400.0","DB1002.12500.0","D2985",null,null,"D2945","DB1002.16400.0","DB1002.16500.0","D2985"]
[null,"D2956","DB1002.12600.0","DB1002.12700.0","D2991",null,null,"D2956","DB1002.16600.0","DB1002.16700.0","D2991"]
[]
[]
["192.168.12.193","读格林晟","写AGV(三楼负极中控 192.168.11.88)","读AGV","写格林晟",null,"192.168.12.198","读格林晟","写AGV(三楼负极中控 192.168.11.88)","读AGV","写格林晟"]
[null,"D2920","DB1002.12800.0","DB1002.12900.0","D2970",null,null,"D2920","DB1002.16800.0","DB1002.16900.0","D2970"]
[null,"D2934","DB1002.13000.0","DB1002.13100.0","D2979",null,null,"D2934","DB1002.17000.0","DB1002.17100.0","D2979"]
[null,"D2945","DB1002.13200.0","DB1002.13300.0","D2985",null,null,"D2945","DB1002.17200.0","DB1002.17300.0","D2985"]
[null,"D2956","DB1002.13400.0","DB1002.13500.0","D2991",null,null,"D2956","DB1002.17400.0","DB1002.17500.0","D2991"]